--- src/wl/sys/wl_cfg80211_hybrid.c	2014-06-26 10:42:08.000000000 +0000
+++ src/wl/sys/wl_cfg80211_hybrid.c	2014-12-30 17:02:13.602127370 +0000
@@ -63,8 +63,13 @@
 static s32 wl_cfg80211_join_ibss(struct wiphy *wiphy, struct net_device *dev,
            struct cfg80211_ibss_params *params);
 static s32 wl_cfg80211_leave_ibss(struct wiphy *wiphy, struct net_device *dev);
+#if LINUX_VERSION_CODE < KERNEL_VERSION(3, 16, 0)
 static s32 wl_cfg80211_get_station(struct wiphy *wiphy,
            struct net_device *dev, u8 *mac, struct station_info *sinfo);
+#else
+static s32 wl_cfg80211_get_station(struct wiphy *wiphy,
+           struct net_device *dev, const u8 *mac, struct station_info *sinfo);
+#endif
 static s32 wl_cfg80211_set_power_mgmt(struct wiphy *wiphy,
            struct net_device *dev, bool enabled, s32 timeout);
 static int wl_cfg80211_connect(struct wiphy *wiphy, struct net_device *dev,
@@ -1387,7 +1392,7 @@
 	key_endian_to_host(&key);
 
 	params.key_len = (u8) min_t(u8, DOT11_MAX_KEY_SIZE, key.len);
-	memcpy(params.key, key.data, params.key_len);
+	memcpy((char *)params.key, key.data, params.key_len);
 
 	if ((err = wl_dev_ioctl(dev, WLC_GET_WSEC, &wsec, sizeof(wsec)))) {
 		return err;
@@ -1421,9 +1426,15 @@
 	return err;
 }
 
+#if LINUX_VERSION_CODE < KERNEL_VERSION(3, 16, 0)
 static s32
 wl_cfg80211_get_station(struct wiphy *wiphy, struct net_device *dev,
                         u8 *mac, struct station_info *sinfo)
+#else
+static s32
+wl_cfg80211_get_station(struct wiphy *wiphy, struct net_device *dev,
+                        const u8 *mac, struct station_info *sinfo)
+#endif
 {
 	struct wl_cfg80211_priv *wl = wiphy_to_wl(wiphy);
 	scb_val_t scb_val;
@@ -2010,9 +2021,15 @@
 
 	notify_ie = (u8 *)bi + le16_to_cpu(bi->ie_offset);
 	notify_ielen = le32_to_cpu(bi->ie_length);
+#if LINUX_VERSION_CODE < KERNEL_VERSION(3, 18, 0)
 	cbss = cfg80211_inform_bss(wiphy, channel, (const u8 *)(bi->BSSID.octet),
 		0, beacon_proberesp->capab_info, beacon_proberesp->beacon_int,
 		(const u8 *)notify_ie, notify_ielen, signal, GFP_KERNEL);
+#else
+	cbss = cfg80211_inform_bss(wiphy, channel, CFG80211_BSS_FTYPE_UNKNOWN, (const u8 *)(bi->BSSID.octet),
+		0, beacon_proberesp->capab_info, beacon_proberesp->beacon_int,
+		(const u8 *)notify_ie, notify_ielen, signal, GFP_KERNEL);
+#endif
 
 	if (unlikely(!cbss))
 		return -ENOMEM;
@@ -2071,7 +2088,26 @@
 			wl_get_assoc_ies(wl);
 			memcpy(&wl->bssid, &e->addr, ETHER_ADDR_LEN);
 			wl_update_bss_info(wl);
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(3, 15, 0)
+			{
+				struct wl_bss_info *bi;
+				u16 bss_info_channel;
+				struct ieee80211_channel *channel;
+				u32 freq;
+
+				bi = (struct wl_bss_info *)(wl->extra_buf + 4);
+				bss_info_channel = bi->ctl_ch ? bi->ctl_ch : CHSPEC_CHANNEL(bi->chanspec);
+
+				freq = ieee80211_channel_to_frequency(bss_info_channel,
+				       (bss_info_channel <= CH_MAX_2G_CHANNEL) ?
+				       IEEE80211_BAND_2GHZ : IEEE80211_BAND_5GHZ);
+
+				channel = ieee80211_get_channel(wl_to_wiphy(wl), freq);
+				cfg80211_ibss_joined(ndev, (u8 *)&wl->bssid, channel, GFP_KERNEL);
+			}
+#else
 			cfg80211_ibss_joined(ndev, (u8 *)&wl->bssid, GFP_KERNEL);
+#endif
 			set_bit(WL_STATUS_CONNECTED, &wl->status);
 			wl->profile->active = true;
 		}
@@ -2629,7 +2665,15 @@
 
 void wl_cfg80211_detach(struct net_device *ndev)
 {
-	struct wl_cfg80211_priv *wl = ndev_to_wl(ndev);
+	struct wl_cfg80211_priv *wl;
+	struct wireless_dev *wdev;
+	
+	wdev = ndev->ieee80211_ptr;
+	if (wdev == NULL) {
+                printk(KERN_ERR "[%s()] in ndev=%p: IEEE80211ptr=%p\n", __FUNCTION__, ndev, wdev);
+                return;
+        }
+	wl = ndev_to_wl(ndev);
 
 	wl_deinit_cfg80211_priv(wl);
 	wl_free_wdev(wl);
--- src/wl/sys/wl_cfg80211_hybrid.c	2015-03-16 14:39:29.899350026 +0100
+++ src/wl/sys/wl_cfg80211_hybrid.c	2015-03-16 14:39:06.732682365 +0100
@@ -1452,7 +1452,11 @@
 		WL_DBG(("Could not get rate (%d)\n", err));
 	} else {
 		rate = dtoh32(rate);
+		#if LINUX_VERSION_CODE >= KERNEL_VERSION(4, 0, 0)
+		sinfo->filled |= BIT(NL80211_STA_INFO_TX_BITRATE);
+		#else
 		sinfo->filled |= STATION_INFO_TX_BITRATE;
+		#endif
 		sinfo->txrate.legacy = rate * 5;
 		WL_DBG(("Rate %d Mbps\n", (rate / 2)));
 	}
@@ -1465,7 +1469,11 @@
 			return err;
 		}
 		rssi = dtoh32(scb_val.val);
+		#if LINUX_VERSION_CODE >= KERNEL_VERSION(4, 0, 0)
+		sinfo->filled |= BIT(NL80211_STA_INFO_SIGNAL);
+		#else
 		sinfo->filled |= STATION_INFO_SIGNAL;
+		#endif
 		sinfo->signal = rssi;
 		WL_DBG(("RSSI %d dBm\n", rssi));
 	}
--- src/wl/sys/wl_dbg.h	2014-06-26 10:42:08.000000000 +0000
+++ src/wl/sys/wl_dbg.h	2014-12-30 17:02:03.840957429 +0000
@@ -55,10 +55,12 @@
 
 #define WL_NONE(args)
 
+#define FORCE_TRACE_LEVEL(fmt, ...) do { printk(KERN_ERR fmt, ## __VA_ARGS__); } while (0) /* ## is GCC specific syntax to remove comma when single arg */
+
 #ifdef BCMDBG_ERR
 #define	WL_ERROR(args)		WL_PRINT(args)
 #else
-#define	WL_ERROR(args)
+#define	WL_ERROR(args)		FORCE_TRACE_LEVEL args
 #endif 
 #define	WL_TRACE(args)
 #define WL_APSTA_UPDN(args)
--- src/wl/sys/wl_linux.c	2014-06-26 10:42:08.000000000 +0000
+++ src/wl/sys/wl_linux.c	2014-12-30 17:02:03.841957446 +0000
@@ -878,7 +878,7 @@ wl_remove(struct pci_dev *pdev)
 static SIMPLE_DEV_PM_OPS(wl_pm_ops, wl_suspend, wl_resume);
 #endif
 
-static struct pci_driver wl_pci_driver = {
+static struct pci_driver wl_pci_driver __refdata = {
 	.name =		"wl",
 	.probe =	wl_pci_probe,
 	.remove =	__devexit_p(wl_remove),
@@ -1270,6 +1270,7 @@ wl_free_if(wl_info_t *wl, wl_if_t *wlif)
 		MFREE(wl->osh, wlif->dev, sizeof(struct net_device));
 #else
 		free_netdev(wlif->dev);
+		wlif->dev = NULL;
 #endif 
 	}
 
@@ -1307,7 +1308,12 @@ wl_alloc_linux_if(wl_if_t *wlif)
 	dev->priv = priv_link;
 #else
 
+#if (LINUX_VERSION_CODE < KERNEL_VERSION(3, 17, 0))
 	dev = alloc_netdev(sizeof(priv_link_t), intf_name, ether_setup);
+#else
+	dev = alloc_netdev(sizeof(priv_link_t), intf_name, NET_NAME_UNKNOWN,
+			   ether_setup);
+#endif
 	if (!dev) {
 		WL_ERROR(("wl%d: %s: alloc_netdev failed\n",
 			(wl->pub)?wl->pub->unit:wlif->subunit, __FUNCTION__));
@@ -1651,11 +1657,7 @@ wl_ioctl(struct net_device *dev, struct
 	}
 
 	WL_LOCK(wl);
-	if (!capable(CAP_NET_ADMIN)) {
-		bcmerror = BCME_EPERM;
-	} else {
-		bcmerror = wlc_ioctl(wl->wlc, ioc.cmd, buf, ioc.len, wlif->wlcif);
-	}
+	bcmerror = wlc_ioctl(wl->wlc, ioc.cmd, buf, ioc.len, wlif->wlcif);
 	WL_UNLOCK(wl);
 
 done1:
@@ -2157,8 +2159,8 @@ wl_start(struct sk_buff *skb, struct net
 	wlif = WL_DEV_IF(dev);
 	wl = WL_INFO(dev);
 
+	skb->prev = NULL;
 	if (WL_ALL_PASSIVE_ENAB(wl) || (WL_RTR() && WL_CONFIG_SMP())) {
-		skb->prev = NULL;
 
 		TXQ_LOCK(wl);
 
@@ -2455,8 +2457,10 @@ wl_monitor(wl_info_t *wl, wl_rxsts_t *rx
 		p80211msg_t *phdr;
 
 		len = sizeof(p80211msg_t) + oskb->len - D11_PHY_HDR_LEN;
-		if ((skb = dev_alloc_skb(len)) == NULL)
+		if ((skb = dev_alloc_skb(len)) == NULL) {
+			WL_ERROR(("in %s:%d [%s()] dev_alloc_skb() failure!", __FILE__, __LINE__, __FUNCTION__));
 			return;
+		}
 
 		skb_put(skb, len);
 		phdr = (p80211msg_t*)skb->data;
@@ -2535,8 +2539,10 @@ wl_monitor(wl_info_t *wl, wl_rxsts_t *rx
 			rtap_len = sizeof(wl_radiotap_ht_brcm_2_t);
 
 		len = rtap_len + (oskb->len - D11_PHY_HDR_LEN);
-		if ((skb = dev_alloc_skb(len)) == NULL)
+		if ((skb = dev_alloc_skb(len)) == NULL) {
+			WL_ERROR(("in %s:%d [%s()] dev_alloc_skb() failure!", __FILE__, __LINE__, __FUNCTION__));
 			return;
+		}
 
 		skb_put(skb, len);
 
@@ -2664,8 +2670,10 @@ wl_monitor(wl_info_t *wl, wl_rxsts_t *rx
 			len += amsdu_len;
 		}
 
-		if ((skb = dev_alloc_skb(len)) == NULL)
+		if ((skb = dev_alloc_skb(len)) == NULL) {
+			WL_ERROR(("in %s:%d [%s()] dev_alloc_skb() failure!", __FILE__, __LINE__, __FUNCTION__));
 			return;
+		}
 
 		skb_put(skb, len);
 
@@ -2990,7 +2998,7 @@ _wl_del_monitor(wl_task_t *task)
 }
 
 void
-wl_set_monitor(wl_info_t *wl, int val)
+wl_set_monitor(wl_info_t *wl, int val) /* public => is called by wlc_hybrid.o_shipped */
 {
 	const char *devname;
 	wl_if_t *wlif;
@@ -3224,42 +3232,75 @@ wl_linux_watchdog(void *ctx)
 #if LINUX_VERSION_CODE < KERNEL_VERSION(3, 10, 0)
 static int
 wl_proc_read(char *buffer, char **start, off_t offset, int length, int *eof, void *data)
+{
+	wl_info_t * wl = (wl_info_t *)data;
 #else
 static ssize_t
-wl_proc_read(struct file *filp, char __user *buffer, size_t length, loff_t *data)
-#endif
+wl_proc_read(struct file *filp, char __user *buffer, size_t length, loff_t *offp)
 {
-	wl_info_t * wl = (wl_info_t *)data;
-	int to_user;
-	int len;
+	wl_info_t * wl = PDE_DATA(file_inode(filp));
+#endif
+	int bcmerror, len;
+	int to_user = 0;
+	char tmp[8];
 
 #if LINUX_VERSION_CODE < KERNEL_VERSION(3, 10, 0)
 	if (offset > 0) {
 		*eof = 1;
 		return 0;
 	}
+#else
+	if (*offp > 0) { /* for example, stop: cat /proc/brcm_monitor0 */
+		return 0; /* 0 <=> EOF */
+	}
 #endif
 
-	if (!length) {
-		WL_ERROR(("%s: Not enough return buf space\n", __FUNCTION__));
-		return 0;
-	}
 	WL_LOCK(wl);
-	wlc_ioctl(wl->wlc, WLC_GET_MONITOR, &to_user, sizeof(int), NULL);
-	len = sprintf(buffer, "%d\n", to_user);
-	WL_UNLOCK(wl);
-	return len;
+	bcmerror = wlc_ioctl(wl->wlc, WLC_GET_MONITOR, &to_user, sizeof(int), NULL);
+ 	WL_UNLOCK(wl);
+
+	if (bcmerror != BCME_OK) {
+		WL_ERROR(("%s: GET_MONITOR failed with %d\n", __FUNCTION__, bcmerror));
+		return -EIO;
+	}
+
+ 	len = snprintf(tmp, ARRAY_SIZE(tmp), "%d\n", to_user);
+	tmp[ARRAY_SIZE(tmp) - 1] = '\0';
+	if (len >= ARRAY_SIZE(tmp)) {
+		printk(KERN_ERR "%s:%d [%s()] output would be truncated (ret=%d)!", __FILE__, __LINE__, __FUNCTION__, len);
+		return -ERANGE;
+	}
+	else if (len < 0) {
+		printk(KERN_ERR "%s:%d [%s()] unable to convert value (ret=%d)!", __FILE__, __LINE__, __FUNCTION__, len);
+		return len;
+	}
+	if (length < len) {
+		printk(KERN_ERR "%s:%d [%s()] user buffer is too small (at least=%d ; user=%d)!", __FILE__, __LINE__, __FUNCTION__, len, (int)length);
+		return -EMSGSIZE;
+	}
+	if (copy_to_user(buffer, tmp, len) != 0) {
+		printk(KERN_ERR "%s:%d [%s()] unable to copy data!", __FILE__, __LINE__, __FUNCTION__);
+		return -EFAULT;
+	}
+	
+#if LINUX_VERSION_CODE >= KERNEL_VERSION(3, 10, 0)
+	*offp += len;
+#endif
+
+ 	return len;
 }
 
 #if LINUX_VERSION_CODE < KERNEL_VERSION(3, 10, 0)
 static int
 wl_proc_write(struct file *filp, const char *buff, unsigned long length, void *data)
+{
+	wl_info_t * wl = (wl_info_t *)data;
 #else
 static ssize_t
-wl_proc_write(struct file *filp, const char __user *buff, size_t length, loff_t *data)
-#endif
+wl_proc_write(struct file *filp, const char __user *buff, size_t length, loff_t *offp)
 {
-	wl_info_t * wl = (wl_info_t *)data;
+	wl_info_t * wl = PDE_DATA(file_inode(filp));
+#endif
 	int from_user = 0;
 	int bcmerror;
 
@@ -3270,7 +3311,11 @@ wl_proc_write(struct file *filp, const c
 	}
 	if (copy_from_user(&from_user, buff, 1)) {
 		WL_ERROR(("%s: copy from user failed\n", __FUNCTION__));
-		return -EIO;
+#if LINUX_VERSION_CODE < KERNEL_VERSION(3, 10, 0)
+ 		return -EIO;
+#else
+		return -EFAULT;
+#endif
 	}
 
 	if (from_user >= 0x30)
@@ -3280,10 +3325,15 @@ wl_proc_write(struct file *filp, const c
 	bcmerror = wlc_ioctl(wl->wlc, WLC_SET_MONITOR, &from_user, sizeof(int), NULL);
 	WL_UNLOCK(wl);
 
-	if (bcmerror < 0) {
+	if (bcmerror != BCME_OK) {
 		WL_ERROR(("%s: SET_MONITOR failed with %d\n", __FUNCTION__, bcmerror));
 		return -EIO;
 	}
+	
+#if (LINUX_VERSION_CODE >= KERNEL_VERSION(3, 10, 0)) && 0 /* no need to update offset because this file should only trigger action... */
+	*offp += length;
+#endif
+
 	return length;
 }
 
@@ -3304,8 +3354,8 @@ wl_reg_proc_entry(wl_info_t *wl)
 	if ((wl->proc_entry = create_proc_entry(tmp, 0644, NULL)) == NULL) {
 		WL_ERROR(("%s: create_proc_entry %s failed\n", __FUNCTION__, tmp));
 #else
-	if ((wl->proc_entry = proc_create(tmp, 0644, NULL, &wl_fops)) == NULL) {
-		WL_ERROR(("%s: proc_create %s failed\n", __FUNCTION__, tmp));
+	if ((wl->proc_entry = proc_create_data(tmp, 0644, NULL, &wl_fops, wl)) == NULL) {
+		WL_ERROR(("%s: proc_create_data %s failed\n", __FUNCTION__, tmp));
 #endif
 		ASSERT(0);
 		return -1;
