# Template file for 'usbarmory-base'
pkgname=usbarmory-base
version=1.0
revision=1
homepage="http://www.voidlinux.eu"
short_desc="Void Linux USBarmory base files"
maintainer="Enno Boland <gottox@voidlinux.eu>"
license="Public Domain"

only_for_archs="armv7l armv7l-musl"
depends="virtual?ntp-daemon usbarmory-u-boot usbarmory-kernel"

do_install() {
	# load LED, CI HDRC i.MX USB binding, and g_ether driver
	vmkdir usr/lib/modules-load.d
	vmkdir usr/lib/modprobe.d
	echo 'options g_ether use_eem=0 dev_addr=1a:55:89:a2:69:41 host_addr=1a:55:89:a2:69:42' > ${DESTDIR}/usr/lib/modprobe.d/g_ether.conf
	for m in ledtrig_heartbeat ci_hdrc_imx g_ether; do
		echo "$m" > ${DESTDIR}/usr/lib/modules-load.d/${m%% *}.conf
	done

	vconf ${FILESDIR}/dhcpcd-usb0.conf
	vsv dhcpcd-usb0
}
