# Template file for 'connman'
pkgname=connman
version=1.4
revision=1
subpackages="$pkgname-devel"
build_style=gnu-configure
configure_args="--enable-pie --enable-threads --enable-ethernet
--enable-wifi --enable-bluetooth --enable-loopback --enable-nmcompat
--enable-polkit --enable-client --with-systemdunitdir=/usr/lib/systemd/system"
makedepends="pkg-config glib-devel dbus-devel iptables-devel gnutls-devel"
fulldepends="dbus bluez wpa_supplicant"
short_desc="Open Source CONNection MANager"
maintainer="Juan RP <xtraeme@gmail.com>"
license="GPL-2"
homepage="http://connman.net/"
distfiles="${KERNEL_SITE}/network/$pkgname/$pkgname-$version.tar.xz"
checksum=469d49d3665e65110c3f380cf0c9d4ea48bc892b0e7dba9e2c9c405fd1acdd84
long_desc="
 The ConnMan project provides a daemon for managing internet connections
 within embedded devices running the Linux operating system. The Connection
 Manager is designed to be slim and to use as few resources as possible,
 so it can be easily integrated. It is a fully modular system that can be
 extended, through plug-ins, to support all kinds of wired or wireless
 technologies. Also, configuration methods, like DHCP and domain name
 resolving, are implemented using plug-ins. The plug-in approach allows for
 easy adaption and modification for various use cases."
