# Template file for 'cubieboard2-base'
pkgname=cubieboard2-base
version=2.5
revision=1
build_style=meta
homepage="http://www.voidlinux.eu"
short_desc="Void Linux Cubieboard2 platform package"
maintainer="Juan RP <xtraeme@voidlinux.eu>"
license="Public Domain"

only_for_archs="armv7l armv7l-musl"
depends="virtual?ntp-daemon cubieboard2-uboot sun7i-kernel linux-firmware-network"

do_install() {
	# Load the sunxi-emac module by default.
	vmkdir usr/lib/modules-load.d
	echo sunxi-emac > ${DESTDIR}/usr/lib/modules-load.d/cubieboard2.conf
	# Set proper perms to some devices.
	vmkdir usr/lib/udev/rules.d
	echo 'KERNEL=="disp|cedar_dev|mali|ump", MODE="0660", GROUP="video"' > ${DESTDIR}/usr/lib/udev/rules.d/50-cubieboard.rules
}
